How to work

- SKMOBO sends sensing data to SKOMOBO+

- tcp server (python) of SKOMOBO+ save the sensing data to file

- web server(apache) read the saved file (jave script)

- web brower show the status

How to start tcp server (python) on SKMOBO+

cd /var/www/html/js

sudo python tcp\_server.py

How to change the status of web browser

edit /var/www/html/js/var.js

bg\_color: blue, green, red, orange

emotion: happy, good, tired, hot

Limitation

- current web files can show only (happy, good) and (high CO2, high temperature)